InS_StArT
PCIMLID.COM
1.0
^Accton EN1203 PCI Ethernet Adapter,PCIMLID.COM,IE0
^Accton EN1207(-TX) PCI fast Ethernet Adapter,PCIMLID.COM,IE0
?This driver supports only PCI machine
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*OIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0()Media Access Type
?NOTE: Media access type will be autodetected on driver's load
TP
TP_NO_LINK_TEST
TP_FULL_DUPLEX
AUI
BNC
@AUTOSENSE
!OIE0(Line_Speed)Line Speed
?NOTE: The default Line speed will be selected on driver's load according to the board (EN1203 or EN1207).
10
100
InS_EnD
