; Cirrus Logic IS-101

[Options]
dwBaudRateMax=256000
nCompression=8
nCompressionBS=8
nCompressionSampleRate=8000
nCompressionUnFrameGSM=0
nCompressionUnShieldDLE=1
nPlaybackVolMin=0
nPlaybackVolMax=255

sStatusRING1=RING1
sStatusRING2=RING2
sStatusRING3=RING3
sStatusRING4=Ring

sCmdInit0=&F&C1&D2S0=0HM0X4
_sCmdEnableDRING=+VDR=1,10
sCmdInactivTimer=S30=
sCmdAnswer=A

nCompressionFrameGSM=0
sCmdDevSpecificInit=&K3
sCmdAmericanCID=+VCID=
sCmdSwitchToDataMode=+FCLASS=0
sCmdDevSpecificVoiceInit=+FLO=2
sVoiceSwitchToVoice=+FCLASS=8
sVoiceBaudRate=
sVoiceCompressGSM=
sVoiceCompressADPCM=+VSM=132,%d,0
sVoiceCompressIMA=+VSM=132,%d,0
sVoiceCompressPCM8U=+VLS=128,%d,0
sVoiceCompressPCM8L=+VSM=128,%d,0
sVoiceCompressPCM16=+VSM=129,%d,0
sVoiceCompressALAW=+VSM=130,%d,0
sVoiceCompressULAW=+VSM=131,%d,0
sVoiceCompressBS=
sVoiceCompressSampleRate=
sVoiceSourceNormal=+VLS=1
sVoiceSourceHandset=+VLS=2
sVoiceSourceMonitor=+VLS=5
sVoiceSourceSpeaker=+VLS=4
sVoiceSourceMic=+VLS=6
sVoiceSourceSpeakerPhone=+VLS=7
sVoiceReceiveVoice=+VRX
sVoiceTransmitVoice=+VTX
sVoiceStopPlay=<h10><h03>
sVoiceStopReceive=<h10><h1B>
sVoiceSilenceDetOff=+VSD=128,0
sVoiceSilenceDetOn=+VSD=%d,%d
iSilenceMin=127
iSilenceMax=129
iSilenceDefault=128
sVoiceTone=+VTS=[%s,%s,%s]
sVoiceToneDetectNone=
sVoiceToneDetectAll=
sVoiceReceiveGain=+VGR=
sVoiceTransmitGain=+VGT=
sVoiceAGC=
sVoiceTADVolume=
sVoiceRingbackGoesAway=+VRA=
sVoiceRingbackNeverCame=+VRN=
sCmdOffHook=H1
sCmdSpeakerOn=M2
sVoiceFlash=+VTS=!

sVoiceSpeakerphoneEnable=+VLS=7;+VSP=1
sVoiceSpeakerphoneDisable=+VSP=0;+VLS=1
sVoiceSpeakerphoneMute=+VLS=1
sVoiceSpeakerphoneUnmute=+VLS=7

sVoiceSourceNone=+VLS=0
sVoiceVTS=+VTS=%s

sVoiceDialSpeed=+VTD=%d
nVoiceDialSpeed=10
nVoiceDialSpeedUnits=10
