; Cirrus Logic CL-MD1414EXX

[Options]

dwBaudRateMax=38400

; Default voice data compression
nCompression=130

; Default number of bits per sample (voice data compression)
nCompressionBS=4

; Sample rate for voice
nCompressionSampleRate=4800

; Retrieve shielded GSM frames (older 'Sportster Vi' modems use it)
;
nCompressionUnFrameGSM=1

; Unshield 10h chars sent by DLE
nCompressionUnShieldDLE=1

nPlaybackVolMin=121
nPlaybackVolMax=131

; Status strings
sStatusOK=OK
sStatusVCON=VCON
sStatusCONNECT=CONNECT

; End Of [voice] Transfer character pair
sStatusMODEM_EOT1=16
sStatusMODEM_EOT2=3

; Different types of rings
sStatusRING=RING
sStatusRING1=RING1
sStatusRING2=RING2
sStatusRING3=RING3
sStatusBUSY=BUSY
sStatusVOICE=VOICE
sStatusNO_ANSWER=NO ANSWER
sStatusNO_DIAL_TONE=NO DIAL TONE
sStatusERROR=ERROR
sStatusNO_CARRIER=NO CARRIER
sStatusCallerID=not used

; Common modem commands
sCmd=AT
sCmdInit0=&F&C1&D2S0=0HM0X4
sCmdEchoOff=E0
sCmdEchoOn=E1
sCmdResponseOff=Q1
sCmdResponseOn=Q0
sCmdUseEnglish=V1
_sCmdEnableDRING=-SDR=7
sCmdInactivTimer=S30=
sCmdAnswer=
sCmdHangup=#VLN=0H0
sCmdDial=D%s
sCmdToneDial=DT%s
sCmdPulseDial=DP%s

; Encapsulate GSM data to frames ( like FE FE <33 bytes> 00 A5 )
nCompressionFrameGSM=0

; Device-specific additional init
sCmdDevSpecificInit=\Q3

; Device-specific additional init (after switching to voice)
sCmdDevSpecificVoiceInit=

sCmdAmericanCID=#CID=

; Data mode selection
sCmdSwitchToDataMode=H

; Switch to online voice mode
sVoiceSwitchToVoice=#VCL=1

; Baud rate = BDR*2400
sVoiceBaudRate=

; Select GSM compression
sVoiceCompressGSM=

; Select ADPCM compression
; Use in conjuction with 'sVoiceCompressBS'
sVoiceCompressADPCM=#VSM=AD4

; Select IMA ADPCM compression, 8000 samples per second
sVoiceCompressIMA=

sVoiceCompressPCM8U=
sVoiceCompressPCM8L=
sVoiceCompressPCM16=
sVoiceCompressALAW=
sVoiceCompressULAW=

; Compression bits-per-sample (affects ADPCM, may be 2, 3 or 4)
sVoiceCompressBS=#VSM=AD

; Voice sample rate select
sVoiceCompressSampleRate=#VSR=

; Select voice source. Default is 'normal'
sVoiceSourceNormal=#VLN=1
sVoiceSourceHandset=#VLN=14
sVoiceSourceMonitor=#VLN=17
sVoiceSourceSpeaker=#VLN=16
sVoiceSourceMic=#VLN=32
sVoiceSourceSpeakerPhone=#VLN=49

; Commands to start receiving and transmitting voice data
sVoiceReceiveVoice=#VRD
sVoiceTransmitVoice=#VPY

sVoiceStopPlay=<h10><h03>
sVoiceStopReceive=<h10><h03>

; Silense detection (should be turned off while detecting caller number)
sVoiceSilenceDetOff=#VCSD=0#VSST=0#VSQT=0
sVoiceSilenceDetOn=#VCSD=1#VSL=%d#VSST=%d
iSilenceMin=121
iSilenceMax=131
iSilenceDefault=127

sVoiceTone=#VTS=[%s,%s,%s]

; Tone detection (should be turned off while detecting caller number)
sVoiceToneDetectNone=#VTD=0,0,0
sVoiceToneDetectAll=#VTD=3F,3F,3F

; Speaker volume / mic sensitivity
sVoiceReceiveGain=#VRL=
sVoiceTransmitGain=#VPL=
sVoiceAGC=
sVoiceRingbackGoesAway=#VRA=
sVoiceRingbackNeverCame=#VRN=
sStatusRING4=RING4
sStatusRINGING=RINGING
sStatusNMBR=NMBR
sStatusNAME=NAME
sStatusDATE=DATE
sStatusTIME=TIME
sStatusMESG=MESG
sCmdDeInit=Z
sCmdOffHook=H1
sCmdSpeakerOn=M2
sCmdEnableHardwareCID=
sCmdDisableHardwareCID=
sVoiceTADVolume=
sVoiceFlash=#VTS=!

sVoiceSpeakerphoneEnable=
sVoiceSpeakerphoneDisable=
sVoiceSpeakerphoneMute=
sVoiceSpeakerphoneUnmute=

sVoiceSourceNone=#VLN=0
sVoiceVTS=#VTS=%s

sVoiceDialSpeed=#VBT=%d
nVoiceDialSpeed=10
nVoiceDialSpeedUnits=10
