; IDC-2814 (Data/Fax)

[Options]
dwBaudRateMax=115200
nCompression=128
nCompressionBS=2
nCompressionSampleRate=8000
nCompressionUnFrameGSM=1
nCompressionFrameGSM=0
nCompressionUnShieldDLE=1
nPlaybackVolMin=0
nPlaybackVolMax=255
sCmdEnableHardwareCID=S95=2
sCmdDevSpecificInit=&K3
sCmdAnswer=*K2 R
sCmdHangup=*K0H
sCmdDevSpecificVoiceInit=
sStatusCallerID=NUMBER:
sStatusRING1=RING1
sStatusRING2=RING2
sStatusRING3=RING3
sStatusRING4=Ring
sCmdInit0=&F&C1&D2S0=0HM0X4
_sCmdEnableDRING=
sCmdInactivTimer=S30=
sCmdSwitchToDataMode=
sVoiceSwitchToVoice=
sVoiceBaudRate=
sVoiceCompressGSM=
sVoiceCompressADPCM=
sVoiceCompressIMA=
sVoiceCompressBS=
sVoiceSourceNormal=
sVoiceSourceHandset=
sVoiceSourceMonitor=
sVoiceSourceSpeaker=
sVoiceSourceMic=
sVoiceSourceSpeakerPhone=
sVoiceReceiveVoice=
sVoiceTransmitVoice=
sVoiceStopPlay=<h10><h03>
sVoiceStopReceive=<h10>!
sVoiceSilenceDetOff=
sVoiceSilenceDetOn=
sVoiceTone=
sVoiceToneDetectNone=
sVoiceToneDetectAll=
sCmdAmericanCID=+VCID=
sVoiceCompressSampleRate=
sVoiceReceiveGain=
sVoiceTransmitGain=
sVoiceAGC=
sVoiceTADVolume=
sVoiceRingbackGoesAway=
sVoiceRingbackNeverCame=
sCmdOffHook=H1
sCmdSpeakerOn=M2
sVoiceFlash=D!

sVoiceSpeakerphoneEnable=
sVoiceSpeakerphoneDisable=
sVoiceSpeakerphoneMute=
sVoiceSpeakerphoneUnmute=

sVoiceSourceNone=+VLS=0
sVoiceVTS=X3DT%s
sVoiceDialSpeed=
nVoiceDialSpeed=10
nVoiceDialSpeedUnits=10
