; ISDN: Intracom Netmod

[Options]
dwBaudRateMax=115200
nCompression=130
nCompressionBS=4
nCompressionSampleRate=8000
nCompressionUnFrameGSM=1
nCompressionFrameGSM=0
nCompressionUnShieldDLE=1
nPlaybackVolMin=0
nPlaybackVolMax=255
sCmdDevSpecificInit=&H1&I0&R2
sCmdDevSpecificVoiceInit=
sStatusRING=RING
sStatusRING1=RING A
sStatusRING2=RING B
sStatusRING3=RING C
sStatusRING4=RING D
sCmdInit0=&F&C1&D2S0=0HM0
_sCmdEnableDRING=
sCmdInactivTimer=
sCmdSwitchToDataMode=
sVoiceSwitchToVoice=
sVoiceBaudRate=
sVoiceCompressBS=
sVoiceSourceNormal=
sVoiceSourceHandset=
sVoiceSourceMonitor=
sVoiceSourceSpeaker=
sVoiceSourceMic=
sVoiceSourceSpeakerPhone=
sVoiceReceiveVoice=
sVoiceTransmitVoice=
sVoiceStopPlay=<h10><h03>
sVoiceStopReceive=<h10>
sVoiceSilenceDetOff=
sVoiceSilenceDetOn=
sVoiceTone=
sVoiceToneDetectNone=
sVoiceToneDetectAll=
sCmdAmericanCID=S82=76
;Disable sCmdAmericanCID=S82=74
sVoiceCompressSampleRate=
sVoiceReceiveGain=
sVoiceTransmitGain=
sVoiceAGC=
sVoiceTADVolume=
sVoiceRingbackGoesAway=
sVoiceRingbackNeverCame=
sCmdOffHook=H1
sCmdSpeakerOn=M2
sVoiceFlash=D!

sVoiceSpeakerphoneEnable=
sVoiceSpeakerphoneDisable=
sVoiceSpeakerphoneMute=
sVoiceSpeakerphoneUnmute=

sVoiceSourceNone=
sVoiceVTS=X3DT%s
sVoiceDialSpeed=
nVoiceDialSpeed=1
nVoiceDialSpeedUnits=100
