; ZyXEL U-336S (data/fax)

[Options]
dwBaudRateMax=115200
nCompression=41
nCompressionBS=4
nCompressionSampleRate=9600
nCompressionFrameGSM=0
nCompressionUnFrameGSM=0
nCompressionUnShieldDLE=1
nPlaybackVolMin=56
nPlaybackVolMax=200
sCmdEnableHardwareCID=S38=2 #G230 &I2
sCmdDisableHardwareCID=&I0
sStatusCallerID=NUMBER:
sStatusRING1=RING1
sStatusRING2=RING2
sStatusRING3=RING3
sStatusRING4=Ring
sStatusNMBR=NUMBER
sStatusNAME=NAME
sStatusDATE=DATE
sStatusTIME=TIME
sCmdInit0=&F&C1&D2S0=0HM0X4
_sCmdEnableDRING=S40.3=1 S40.4=1 S40.5=1 S40.6=1
sCmdInactivTimer=S30=
sCmdSwitchToDataMode=
sCmdAnswer=A
sCmdHangup=H
sVoiceSwitchToVoice=
sVoiceBaudRate=
sVoiceCompressGSM=
sVoiceCompressADPCM=
sVoiceCompressIMA=
sVoiceCompressBS=
sVoiceSourceNormal=
sVoiceSourceHandset=
sVoiceSourceMonitor=
sVoiceSourceSpeaker=
sVoiceSourceMic=
sVoiceSourceSpeakerPhone=
sVoiceReceiveVoice=
sVoiceTransmitVoice=
sVoiceStopPlay=<h10><h03>
sVoiceStopReceive=<h10>!
sVoiceSilenceDetOff=
sVoiceSilenceDetOn=
iSilenceMin=1
iSilenceMax=31
iSilenceDefault=15
sVoiceTone=
sVoiceToneDetectNone=S39.6=0
sVoiceToneDetectAll=S39.6=1
sCmdDevSpecificInit=&H3
sCmdDevSpecificVoiceInit=
sVoiceCompressSampleRate=
sCmdAmericanCID=S40.2=1
sVoiceReceiveGain=
sVoiceTransmitGain=
sVoiceAGC=
sVoiceTADVolume=
sVoiceRingbackGoesAway=
sVoiceRingbackNeverCame=
sCmdOffHook=H1
sCmdSpeakerOn=M2
sVoiceCompressALAW=
sVoiceCompressULAW=
sVoiceFlash=

sVoiceSpeakerphoneEnable=
sVoiceSpeakerphoneDisable=
sVoiceSpeakerphoneMute=
sVoiceSpeakerphoneUnmute=

sVoiceSourceNone=
sVoiceVTS=X3DT%s
sVoiceDialSpeed=
nVoiceDialSpeed=10
nVoiceDialSpeedUnits=10
