Some models ship with 1 MB, some with 2 MB.  A 120-pin video DIMM connector allows the use of +5V EDO DRAM, +3.3V SDRAM and +3.3V SGRAM.  Upgrades  are possible by replacing the DIMM.  The 4 MB configuration is possible only with SDRAM or SGRAM.

NOTE: In the 800x600 resolution at a vertical refresh rate of 75 Hz, the 2 MB EDO will only provide 16 bit video (32,768 colors).  At slower refresh rates, or with SGRAM or SDRAM installed,  24 bit video (16.7 million colors) is available in the 800x600 resolution.

Supports resolutions from 640x480 to 1280x1024.