SCSI: HDI-30
Serial Ports: 1
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: AAUI-15
Machine Gestalt ID: 72
PRAM Battery: service center replacement only

Minutiae:

40 and 56 MB configurations are only possible when the ***NO LONGER MANUFACTURED***  NUpowr processor upgrade card is installed.  The 117 MHz and 167 MHz cards both had 8 MB onboard, and the 183 MHz version had 24 MB onboard.

Apple sometimes advertises this as a 50 MHz machine, since the clock speed is doubled inside the processor chip.  However, all I/O to the processor is done at 25 MHz. 

9.5” FSTN passive matrix LCD - 4 bit (16 Grays) Display.

One of the configurations sold by Apple contains 12 MB of memory.  This configuration requires the removal of the factory-installed 8 MB memory module in order to upgrade to a larger capacity memory module.

Serial Port with the phone icon supports synchronous modems, with handshaking on both the output and input.

Has 2 MB ROM and a 1.44 MB SuperDrive.