SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: optional
Machine Gestalt ID: ??

Minutiae:

Due to conflicting information from UMAX, NewerRAM is recommending the use of 5 volt (not 3.3 volt) EDO (extended data out) memory.  UMAX’s website says either FPM (fast paged mode) or EDO will work.  Some of their  manuals say only EDO will work.  There is no technical reason for us to recommend EDO.  The recommendation is made simply because Technical Support was getting too many calls from people convinced that they had been sent the wrong memory when they received FPM DIMMs.

Memory system is non-interleaved.

Manufactured by UMAX Computer Corporation
Toll-free tech support at 1-888-600-4400
Online system support at www.supermac.com