SCSI: DB-25
Serial Ports: 2
Sound Output: 16-bit stereo 44.1 KHz sample rate
ADB: 2
Ethernet:  10baseT
Machine Gestalt ID: ???
PRAM Battery: unknown

Minutiae:

A price advantage may be available by using 5 volt (not 3.3 volt) EDO (extended data out) instead of FPM (fast paged mode) memory.  However, you will not derive any performance benefits by using EDO DIMMs.   Call your NewerRAM rep for details.

Processor card cache bus runs at 125 MHz.  In addition to the 512 K backside cache, the motherboard has 512K of L3 cache

Manufactured by: 

PIOS Computer AG
Borsigstr. 5
D-31135 Hildesheim
Germany
Tel. +49 - 5121 - 7533-0
Fax  +49 - 5121 - 7533-75
website: http://www.pios.de/
email: info@pios.de