Supported System Software: 7.5.2, 7.5.3
SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: AAUI, 10baseT built-in or upgrade to Newer Technology 7ET-PCI10/100
Machine Gestalt ID: 67

Minutiae:

Upgraded with one DIMM at a time.

Can be accelerated with Newer Technology's Eddy Award winning "PowerClip 604™", part # 7MC604.  The PowerClip has over 100 different speed settings which allow the PowerMac 9500 to be set at speeds of up to 175MHz. Typically the 9500/132 will be set to something between 150MHz and 164MHz. The PowerClip is slotless.

Can interleave memory for approximately 10-30% faster RAM access.  For the fastest speed, sockets A1 & B1, A2 & B2...A6 & B6 should contain identical capacity DIMMs.

Original enabler: 701 v1.0

Serial Port with the phone icon supports synchronous modems, with handshaking on both output and input supported.

Has 4MB ROM and a 1.44MB SuperDrive.