BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Houston Instruments B-sized PC625      --
--                          plotter                                    --
--                                                                     --
-------------------------------------------------------------------------
-- 10-15-89 JSM Added prefix & suffix string, port information, etc.
-- 7-17-87 TT - Set COM1 as release port
-- 7-06-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 1  -- communications port number:
--  0 = custom port configuration, see documentation for more information
--  1 = COM1
--  2 = COM2
-- -1 = LPT1 (using BIOS) \
-- -2 = LPT2 (using BIOS)  - these can be redirected by most networks
-- -3 = LPT3 (using BIOS) /  (10k bits per second)
-- -4 = LPT1 (using direct I/O) \
-- -5 = LPT1 (using direct I/O) - These are very fast, but do not work
--                                on all machines, and cannot be redirected
--                                by any networks
--                                (80k bits per second)
   

1  'B A A4 A3 BS '   -- Paper Size Words (must have space at end)
105 0 1 1  0  0      -- XY axis rotation flag for each paper size

-- Paper sizes
201          0       0   15000    9800  -- B
202          0       0    9800    6380  -- A
203          0       0   10460    6180  -- A4
204          0       0   14360   10480  -- A3
205          0       0   14500    9800  -- BS
 
--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  6  1 1

--    +-----+---------- X,Y plotter units per inch
--    V     V
103 1000  1000

104 38               -- Max pen speed

-- Prefix string to sent before plot (use to setup plotter, switches, etc)
--29  ''
-- Suffix string to be sent after plot
--30  ''

END DDIF
END
