BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Hewlett-Packard Draft Master plotter   --
--         ( A , B , C , D , E-size) (used with HP7585B.DEV)           --
--                       HP7595  DraftMaster I                         --
--                       HP7596  DraftMaster II                        --
-------------------------------------------------------------------------
-- 10-15-89 JSM Added prefix & suffix string, port information, etc.
-- 05-04-88  ALA - Update paper sizes again!!
-- 07-17-87  TT  - Set COM1 as release port
-- 07-09-87  KMM - Updated the paper sizes
-- 07-06-87  TT  - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 1  -- communications port number:
--  0 = custom port configuration, see documentation for more information
--  1 = COM1
--  2 = COM2
-- -1 = LPT1 (using BIOS) \
-- -2 = LPT2 (using BIOS)  - these can be redirected by most networks
-- -3 = LPT3 (using BIOS) /  (10k bits per second)
-- -4 = LPT1 (using direct I/O) \
-- -5 = LPT1 (using direct I/O) - These are very fast, but do not work
--                                on all machines, and cannot be redirected
--                                by any networks
--                                (80k bits per second)
   

1  'D A B C E A4 A3 A2 A1 A0 BS' -- Paper size string (must have space at end)
105 0 0 0 0 0  0  0  0  0  0  0  -- XY axis rotation flag for each paper size
                                 -- No rotation for DraftMaster.
                                 -- Plotter will figure out which is X.
-- Paper sizes
201     -16086  -10480   16086   10480  --D  mounted vertically
202      -4900   -3164    4900    3164  --A  mounted horizontally
203      -7474   -4934    7474    4934  --B  mounted vertically
204     -10500   -7410   10500    7410  --C  mounted horizontally
205     -21095  -16632   21095   16632  --E  mounted vertically
206      -5140   -3080    5140    3080  -- A4
207      -7120   -5140    7120    5140  -- A3
208     -11080   -7080   11080    7080  -- A2
209     -15500  -11080   15500   11080  -- A1
210     -22660  -16180   22660   16180  -- A0
211      -7250   -4900    7250    4900  -- BS

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  8  1 1

--    +-----+------ X,Y plotter units per inch
--    V     V
103 1016  1016

104 60           -- Max pen speed

-- Prefix string to sent before plot (use to setup plotter, switches, etc)
--29  ''
-- Suffix string to be sent after plot
--30  ''

END DDIF
END
