BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Hewlett-Packard Draft Pro plotter      --
--                          (D-size) (used with HP7580B.DEV)           --
--                                                                     --
-------------------------------------------------------------------------
-- 10-15-89 JSM Added prefix & suffix string, port information, etc.
-- 5-23-88 ALA- Fix the paper sizes.
-- 7-17-87 TT - Set COM1 as release port
-- 7-06-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 1  -- communications port number:
--  0 = custom port configuration, see documentation for more information
--  1 = COM1
--  2 = COM2
-- -1 = LPT1 (using BIOS) \
-- -2 = LPT2 (using BIOS)  - these can be redirected by most networks
-- -3 = LPT3 (using BIOS) /  (10k bits per second)
-- -4 = LPT1 (using direct I/O) \
-- -5 = LPT1 (using direct I/O) - These are very fast, but do not work
--                                on all machines, and cannot be redirected
--                                by any networks
--                                (80k bits per second)
   

1  'C A2 A B D A4 A3 A1 BS  '   -- Paper size string (must have space at end)
105 0  0 1 0 0 1  0  0  0       -- XY axis rotation flag for each paper size

-- Paper sizes
201          -10500   -7464    10500    7464     -- C
202          -11080   -7080   11080    7080     -- A2
203           -4900   -3190    4900    3190     -- A
204           -7500   -4988    7500    4988     -- B
205          -16160  -10480   16160   10480     -- D
206           -5140   -2990    5140    2990     -- A4
207           -7120   -5140    7120    5140     -- A3
208          -15500  -11080   15500   11080     -- A1
209           -7250   -4900    7250    4900     -- BS

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  8  1 1

--    +-----+------ X,Y plotter units per inch
--    V     V
103 1016  1016

104 60           -- Max pen speed

-- Prefix string to sent before plot (use to setup plotter, switches, etc)
--29  ''
-- Suffix string to be sent after plot
--30  ''

END DDIF
END
