BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Ioline 3700 series plotters            --
--                                                                     --
--                                                                     --
-------------------------------------------------------------------------
-- 10-15-89 JSM Added prefix & suffix string, port information, etc.
-- 7-21-87 SJO  Corrected Paper Sizes
-- 7-17-87 TT - Set COM1 as release port
-- 7-06-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 1  -- communications port number:
--  0 = custom port configuration, see documentation for more information
--  1 = COM1
--  2 = COM2
-- -1 = LPT1 (using BIOS) \
-- -2 = LPT2 (using BIOS)  - these can be redirected by most networks
-- -3 = LPT3 (using BIOS) /  (10k bits per second)
-- -4 = LPT1 (using direct I/O) \
-- -5 = LPT1 (using direct I/O) - These are very fast, but do not work
--                                on all machines, and cannot be redirected
--                                by any networks
--                                (80k bits per second)
   

1  'A B C D E  '  -- Paper size string (must have space at end)
105 0 0 0 0 0     -- XY axis rotation flag for each paper size

-- Paper sizes
201          0       0    3500    2700  -- A
202          0       0    5850    3750  -- B
203          0       0    7800    5850  -- C
204          0       0   11900    7800  -- D
205          0       0   16000   12000  -- E

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  1  1 1

--    +-----+------ X,Y plotter units per inch
--    V     V
103  400   400

104 8            -- Max pen speed

-- Prefix string to sent before plot (use to setup plotter, switches, etc)
--29  ''
-- Suffix string to be sent after plot
--30  ''

END DDIF
END
