BEGIN DDIF

------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for IBM Professional Graphics display     --
--                          board and MATROX PG-640 Graphics board    --
--                          (640 pixels by 480 pixels)                 --
------------------------------------------------------------------------

--
-- 6-24-87  TT - Upgraded for rev 3.0
-- 03/15/87      Fix line 101 and add lines 3,4,5
-- 04/25/86
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

-- Graphics Device Driver --

-- The file name to echo commands to is given on code line 1.  To activate
-- this feature remove the '--' comment characters in front of the 1 or put 
-- in a '--' to deactivate it.  The file can then be displayed by copying it
-- to the CGB device. Ie. C>COPY /B PG.CGB CGB:

--1 PG.CGB

-- Color Table Definition

--    +---Index 0 is the graphics background color (000 = black)
--    |
--    |                 Entity Color Table
--    |                 ------ ----- -----
--    |                 Color Table Values (RGB) (0-9)(A-F)
--    |                 (0 - 9 & A   0 = Dimmest, A = Brightest)
--    V
--    0   1   2   3   4   5   6   7   8   9  10  11  12  13  14  15
--    +---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |   |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V   V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB 
2   "100 600 060 006 660 067 606 667 333 900 090 009 880 09A A0A 999" --Documented no bkg

--          Starting Shading Color Table Values (RGB)
--          -------- ------- ----- ----- ------ -----
--    0   1   2   3   4   5   6   7   
--    +---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB
3   "000 800 080 008 880 088 808 000"

--                Dark Shading Color Increments (RGB)
--                ---- ------- ----- ---------- -----
--    0   1   2   3   4   5   6   7
--    +---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB
4   "111 100 010 001 110 011 101 111"

--               Light Shading Color Increments (RGB)
--               ----- ------- ----- ---------- -----
--    0   1   2   3   4   5   6   7
--    +---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB
5   "111 011 101 110 001 100 010 111"

--  +-- Cursor character number
--  V   
101 95

-- 16 bit line font patterns           (Entity ident hilite font)
--                                                  |
--                                                  V
--    1     2    3      4      5      6      7      8
102 6168   4080  8184  32742  32663  15420    15   26214

-- Beep definition line in duration,frequency divisor pairs
-- (divisor = 1193180/desired freq, ie divisor for 400hz = 2983)
--
-- Up to 10 pairs may be given.
-- This line is optional and may be commented out to get the default beep.

103 4 4200 2 3800 1 3400 1 3000 1 2600 1 2200 1 1800 4 1400 2 1000 2 800

--    +-----+-- X,Y Screen pixels per inch
--    V     V
301 70.20 70.20

END DDIF
END
