--                      DLISTON.DEF

-- The information provided to the Vermont Microsystems Driver by this file
-- is as follows:
--      1. Entry 101: The cursor character value, 95.
--      2. Entry 103: Display List saving is implemented, 1.

-- The complete list of data that could be provided to the Device Driver is
-- shown with the entry written as a comment and example if it is not 
-- implemented. 
-- The reason data is not provided for the Device Driver is because the 
-- Driver already contains default values. 
-- If the CV user wants to change the default values, then the
-- corresponding data may be initialized accordingly.


BEGIN DDIF

-- RGB color table values. Read by cv_sload.
   2 "100 600 060 006 660 067 606 667 333 900 090 009 880 09A A0A 999"

-- Starting RGB values for the shading color table. Read by cv_sload.
-- 3 "000 800 080 008 880 088 808 000"

-- RGB increments for the dark shades of each color. Read by cv_sload.
-- 4 "111 100 010 001 110 011 101 111"

-- RGB increments for the light shades of each color. Read by cv_sload.
-- 5 "111 011 101 110 001 100 010 111"

-- Cursor Char number. Read by cv_iload.
   101 95

-- Up to 8 text font patterns. Read by cv_iload. Set to none
   102  6168  4080  8184  32742  32663  15420  15  26214

-- 103  
-- Dlist implemented. Read by cv_iload.
   104 1
-- Number of 16K pages of expanded memory to be allocated for dlist.
-- Default is 64 pages: 1 meg
   109 64
-- X and Y pixels per inch for graphics screen. Read by cv_rload.
   301 98.0 99.0 

END DDIF

END

