BEGIN DDIF
------------------------------------------------------------------------------
-- DGIS Device Information File					            --
------------------------------------------------------------------------------
-- 07-05-90
--
--	  +------- Graphics device description
--	  |
--	  V
1 "4D Graphics DGIS"

--  +--------- 0 = use default color table
--  |	       1 = use specified color map (not implemented yet)
--  |          
--  |  +------ 0 = no CGA capability
--  |  |       1 = use CGA/EGA emulation hardware
--  |  |       2 = use alternate CGA/EGA monitor
--  |  |
--  |  |  +--- 0 = use default screen pixel density
--  |  |  |    1 = use specified screen pixel density
--  V  V  V
101 0  1  1
--
--		 Color Table Values (intensity,red,green,blue)
--
--	 0	     1		2	    3		4
--	 +-----------+----------+-----------+-----------+
--	 |	     |		|	    |		|
--	 V	     V		V	    V		V
--   I	R G B	I   R G B   I  R  G B	I  R G	B   I  R  G B
102 255 3 3 3  255 14 0 0  255 0 14 0  255 0 0 14  255 12 12 0

--	  5	       6	    7		 8	    9
--	  +------------+------------+------------+----------+
--	  |	       |	    |		 |	    |
--	  V	       V	    V		 V	    V
--   I	 R G  B   I  R	G  B   I   R  G  B   I	R G B	I  R G B
103 255 12 0 12  255 0 12 12  255 12 12 12  127 0 0 0  127 7 0 0

--	 10	    11	       12	  13	     14
--	 +----------+----------+----------+----------+
--	 |	    |	       |	  |	     |
--	 V	    V	       V	  V	     V
--   I	R G B	I  R G B   I  R G B   I  R G B	 I  R G B
104 127 0 7 0  127 0 0 7  127 6 6 0  127 6 0 6	127 0 6 6

--	 15
--	 +
--	 |
--	 V
--   I	R G B
105 127 6 6 6

--  If you expect items which are measured in screen inches (Gleep size,
--  point size, cpl axis size, etc) to be the correct size you MUST set
--  the following values for your particular monitor/card combination
--
--    +------+--X,Y Screen Pixels per inch
--    |      |
--    V      V
301 90.62 92.53         -- 1024x768 on 16" monitor

--   GRAPHICS DRIVER CONFIG FLAGS.
--  *** DO NOT CHANGE THIS LINE ***
--  0 in a line number field means not used.
--    +-------------------------------- 0 = low res   ,  1 = high res.
--    |    +--------------------------- Color lookup table line number
--    |    |    +---------------------- Start shade color table line number
--    |    |    |    +----------------- Dark shade color table line number
--    |    |    |    |    +------------ Light shade color table line number
--    |    |    |    |    |    +------- Number of dsplist 16k's line number
--    |    |    |    |    |    |    +-- Dsplist o/f file name line number
--    |    |    |    |    |    |    |
120   0    0    0    0    0    0    0

END DDIF
END
