BEGIN DDIF
----------------------------------------------------------
-- IBM EGA DEVICE INFORMATION FILE                      --
--                                                      --
----------------------------------------------------------

-- DIGITAL MONITOR COLOR INFORMATION
-- pallete number to be used for GCD color number:
--   0  1  2  3  4  5  6  7  8  9  10 11 12 13 14 15
--   v  v  v  v  v  v  v  v  v  v  v  v  v  v  v  v
102 00 04 02 01 06 03 05 07 08 12 10 09 14 11 13 15 -- standard colors

-- PIXEL DENSITIES (you must set these for your monitor)
-- for most 13" monitors, pixels in x dimension would be xres/8.5
--                        pixels in y dimension would be yres/6.375
--    +-----+-- X,Y SCREEN PIXELS/PER INCH
--    V     V
301 63.77 50.24

--   GRAPHICS DRIVER CONFIG FLAGS.
--  *** DO NOT CHANGE THIS LINE ***
--  0 in a line number field means not used.
--    +-------------------------------- 0 = low res   ,  1 = high res.
--    |    +--------------------------- Color lookup table line number
--    |    |    +---------------------- Start shade color table line number
--    |    |    |    +----------------- Dark shade color table line number
--    |    |    |    |    +------------ Light shade color table line number
--    |    |    |    |    |    +------- Number of dsplist 16k's line number
--    |    |    |    |    |    |    +-- Dsplist o/f file name line number
--    |    |    |    |    |    |    |
120   0  102    0    0    0    0    0

END DDIF
END
