BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Hewlett-Packard 7580B plotter (D size) --
--                          (7580A not supported)                      --
-------------------------------------------------------------------------
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

-- COMMUNICATIONS PARAMETERS
--   +-- commications port number  0        = use default file name below
--   |				   1 to  4  = SERIAL ports COM1 to COM4 
--   |				  -1 to -3  = PARALLEL ports LPT1 to LPT3
--   |				  -4 to -6  = PARALLEL ports LPT1 to LPT3
--   |				              (using direct, hardware I/O)
--   |	 SERIAL PORT PARAMETERS (default = 9600 baud, none, 1 stop, 8 data)
--   |   +------------------------------------------- BAUD RATE   
--   |   |  +------------------------------ PARITY     0 =  9600	          
--   |   |  |  +---------------- STOP BITS   0 = NONE  1 =   300           
--   |   |  |  |  +-- DATA BITS   0 = 1	     1 = EVEN  2 =  1200           
--   |   |  |  |  |    0 = 8	  1 = 1	     2 = ODD   3 =  2400           
--   |   |  |  |  |    7 = 7	  2 = 2	 	       4 =  4800           
--   |   |  |  |  |    8 = 8			       5 =  9600           
--   |   |  |  |  |			               6 = 19200           
--   |   |  |  |  |			               7 = 38400           
--   |   |  |  |  |        			       8 = 57600
--   v   v  v  v  v
101  2

-- DEFAULT FILE NAME  to use if communication port is '0' (above)
-- and file name or port number is not given at plot time
19 PD_PLOT.HP

1  'A B C D E A4 A3 A2 A1 A0 BS  '  -- Paper size string (must have space at end)
105 1 0 0 0 0 1  0  0  0  0  0      -- XY axis rotation flag for each paper size

-- Paper sizes
201           -4900   -3190    4900    3190     -- A
202           -7500   -4900    7500    4900     -- B
203           -9990   -7980    9990    7980     -- C
204          -16060  -10460   16060   10460     -- D
205          -21000  -16580   21000   16580     -- E
206           -5230   -3090    5230    3090     -- A4
207           -7180   -5240    7180    5240     -- A3
208          -10680   -7660   10680    7660     -- A2
209          -15520  -11160   15520   11160     -- A1
210          -22190  -16145   22190   16145     -- A0
211           -7250   -4900    7250    4900     -- BS

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  8  1 1

--    +-----+------ X,Y plotter units per inch
--    V     V
103 1016  1016

104 60           -- Max pen speed

-- PREDEFINED COMMAND STRINGS
-- format for these must be as follows:
--    +-- string name, up to eight characters, ending with a space
--    |      +-- plotter commands up to 55 characters.  Any characters
--    |      |   allowable, control codes must be formatted in '#n#'-style
--    |      |   notation.  This data will be sent verbatim to the plotter
--    |      |   so any base conversion or bias must already be incorporated
--    v	     v
-- 'NAME     plotter command data'

20 'RESET    IN;'
21 'OFFLINE  NR;'
22 'FEED     PG;'
--23
--24
--25
--26
--27 
--28

-- PREFIX AND SUFFIX STRINGS:
-- data must be in quotes (single or double) names are case sensitive
-- EXAMPLE:  'RESET "some plotter data" FEED'
-- NAME(s) of Predefined string(s) or data to send BEFORE PLOT
--29  ''
-- NAME(s) of Predefined string(s) or data to send AFTER PLOT
--30  'FEED'

END DDIF
END
