–	Maximum durability under shock loading