•	The result possible cracking of the raceway and caster failure