•	Operating temperature range