"A)scii
",1,IA,,,,,,0.92,,,,
"B)atch Ymodem (DSZ)
",1,S,8,,B,1024,,0.90,,1=E,".\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow sb -k [FILE]",".\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow rb [FILE] -p"
"C)rc Xmodem
",1,IC,8,,,128,,0.78,,,,
"G) YmodemG
",1,S,8,R,,1024,,0.90,,,".\XFER\QMXFER.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p G -n [NODE]",".\XFER\QMXFER.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p G -n [NODE]"
"K)ermit
",1,S,,,,128,F,0.78,,,".\XFER\PCKERMIT.EXE -s [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31",".\XFER\PCKERMIT.EXE -r -a [FILE] -l [PORT] -c -b [BAUD] -p [PARITY] -m 31"
"M)pt (formerly, PUMA)
",1,S,8,,B,1024,,0.95,,1=E,".\XFER\MPT.EXE S[BAUD] P[PORT#] HS LXFER-[NODE].DEF N+ A+ O- B- X+ S [FILE]",".\XFER\MPT.EXE S[BAUD] P[PORT#] HS LXFER-[NODE].DEF N+ A+ O- B- X+ R [FILE]"
"W)indowed Xmodem
",1,S,,,,128,,0.78,,,".\XFER\WXMODEM.COM -s -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]",".\XFER\WXMODEM.COM -r -f [FILE] -l [PORT] -c -b [BAUD] -p W -n [NODE]"
"X)modem
",1,IX,8,,,128,,0.78,,,,
"Y)modem (1K Xmodem)
",1,IY,8,,,1024,,0.87,,,,
"Z)modem (Batch)
",1,S,8,,B,1024,,0.95,,1=E,".\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow sz [FILE]",".\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow rz [FILE] -p"
"#)Zmodem doored to (example for sysop)
",10,D,8,,B,1024,,0.95,,4=E=A,".\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow sz [FILE]",".\XFER\DSZ.COM port [PORT#] speed [BAUD] handshake slow rz [FILE] -p"
"N)one - Cancel

Select Protocol",1,IN,,,,,,,,,,
