Hello:

This is the calibration for the Epson Stylus at 720 dpi.  It reduces the maximum density to 65%.  

To install it, login as root, then look in the directory /usr/local/lib/ColorXPrinter/Printers

There should be in here another directory that is the same name as the name you gave to the printer when you installed it. Copy the file into this folder, then rename it to "basic.calibration"

epson_stylus_720.calibration<----Calibration file for EpsonStylus @ 720 DPI

Run the eXTRAPRINT.app and choose "Server->Shutdown"

Print again, and the ink saturation problems should go away.

Finally, we are making a new  PPD which eliminates the PostScript sreening option. Due to limitations of DPS, high resolutions halftone screens in color are not possible. Our Floyd Steinberg screening is much better anyway, so it shouldn't be missed.

Best regards, 

John