Wacom Tablet Driver 1.2e (Beta)
24th August 1994

This tablet driver originated from Talus Corp. but was too buggy to be considered useful. Cambridge Animation modified the driver so that it is stable on i486 machines and reasonably stable on Pentium machines.

The driver is still considered to be in beta as the Pentium version has not proved itself totally reliable.

Installation

Ensure the disk Tablet_1.2e is in the disk drive.
Run the Configure.app in /NextAdmin
Select the Mouse options.
If there is already a Wacom Serial Tablet entry, select it and click on Remove.
Click on Add. This will bring up a panel of drivers currently recognized. There may
already be a tablet driver in the list, if so ignore it.
Click in Install Driver. This will bring up an open panel. Scroll to the left most column and select Tablet_1.2e then WacomTablet.config and click on Ok. This will add a new Wacom Tablet driver to the list of available devices. Select the bottom most one and click on Add....
Click on Done. This will take you to the summary panel.
Click on Save.
Log out and reboot. After logging in, open /usr/adm/messages and check near the bottom for the line 'Wacom Tablet Device Driver. Version 1.2e'. If this is present and the tablet appears to work then all is well.

Recent Changes

1.2c:	First CAS beta release. Fixes race problems on 486 machines
1.2d:	Second beta release. Button defaults made sensible
1.2e:	Minor internal changes