Pages Per Minute:  20 max
DPI (max):  600
Interface:  LocalTalk, RS-232/422 serial, 1284 Bidirectional parallel, Ethernet, SCSI
Page Description Language:  PostScript Level 3
Minimum Engine Life (pgs):  650,000

Minutiae:

1 SIMM socket.  Ships with 16MB soldered on the motherboard.

The user guide for this printer has conflicting info on which direction the SIMM should be installed.  The text says the SIMM notch should be on the left, but the illustration shows it on the right.  The notch should be on the left.  The illustration is in error.

Energy Star:
EPA Energy Star-compliant.