24 bit video (millions of colors) is only supported up to the 1024x768 resolution on 21” monitors.

Machine ships with 2 MB of SGRAM soldered onto the logic board.  The video RAM can be expanded to 4 MB or 6 MB with the addition of either a 2 MB or a 4 MB SO-DIMM (small outline dual inline memory module).