SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: 10baseT
Machine Gestalt ID: 515
PRAM Battery: 4.5V alkaline (Rayovac 840)

Minutiae:

This system is not sold in the U.S.

Only supports 3.3 volt EDO (extended data out) DIMMs.  It does not support interleaved memory.  The three DIMM sockets are NOT identical.  The first socket can only accept up to 32 MB DIMMs.  The other two sockets can accept up to 64 MB DIMMs.  The maximum memory is therefore 160 MB.

Has 4MB ROM and a 1.44MB SuperDrive.