SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: AAUI, 10baseT
Machine Gestalt ID: 67
PRAM Battery: 3.6V lithium (Maxell ER3S, Radio Shack 23-026)

Minutiae:

A price advantage may be available by using 5 volt (not 3.3 volt) EDO (extended data out) instead of FPM (fast paged mode) memory.  However, you will not derive any performance benefits by using EDO DIMMs.   Call your NewerRAM rep for details.

Upgraded with one DIMM at a time.

Processor board contains two PowerPC 604e processors.

The 512K of Level 2 Cache on the motherboard is not upgradeable.

Can interleave memory for approximately 10-30% faster RAM access. 

Serial Port with the phone icon supports synchronous modems, with handshaking on both output and input supported.

Has 4MB ROM and a 1.44MB SuperDrive.