SCSI: none
Serial Ports: 1
Sound Output: mono 16 bit.
ADB: see below
Ethernet: see below
Machine Gestalt ID: 118
PRAM Battery: service center replacement only

Minutiae:

9.5” active matrix LCD - 16-bit (thousands of colors) Display.

Has a 152-pin PDS (Processor Direct Slot) connector for connecting to the Duo Docks.

Serial Port with the phone icon supports synchronous modems, with handshaking on both the output and input.

Has 4 MB ROM.