Has 512KB of VRAM soldered to the motherboard.

Has one VRAM SIMM socket.

Unless System 7.5.3 or higher is installed, a display adapter is required to use Multiple Scan Monitors at 832 x 624 resolution.