Unless System 7.5.3 or higher is installed, a display adapter is required to use Multiple Scan Monitors at 832 x 624 resolution.