SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: 10BaseT, AAUI-15
Machine Gestalt ID: ??

Minutiae:

Upgraded with one DIMM at a time.

Ships with a minimum of 16MB (two 8MB, or one 16MB DIMM) of RAM installed.

Can interleave memory for approximately 10-30% faster RAM access.  For the fastest speed, sockets A1 & B1, A2 & B2...A4 & B4 should contain identical capacity DIMMs.

Has 4096K ROMs and a 1.44MB SuperDrive.

Serial Ports with the phone icon and printer icon support synchronous modems, with handshaking on both output and input supported. Both Serial ports can be used with Apple's GeoPort telecom adaptor.

Energy Star compliant 

Three high-performance PCI expansion slots compatible with all PCI 2.0 specification-compliant cards (or Two PCI expansion slots and two NuBus expansion slots).

Manufactured by:
Power Computing Corporation
1-800-769-5917
info@powercc.com
http://www.powercc.com