SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: AAUI, 10baseT
Machine Gestalt ID: ???

Minutiae:

Upgraded with one DIMM at a time.

Accelerate performance through the addition of a NewerRAM 256KB Cache DIMM, part # CC256B.

Ships with a minimum of 8MB of RAM installed.

Original enabler: 701 v1.1

Serial Port with the phone icon supports synchronous modems, with handshaking on both output and input supported.

Has 4MB ROM and a 1.44MB SuperDrive.

Manufactured by:
Power Computing Corporation
1-800-769-5917
info@powercc.com
http://www.powercc.com