Video is provided by means of a 2MB PCI video card. To achieve greater color depths the card accepts a 2MB VRAM daughtercard, NewerRAM part # VR2MB.

This computer has no built-in Video input, Dual-stream Video output,or DAV slots.