SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: optional
Machine Gestalt ID: ??

Minutiae:

NewerRAM recommends the use of 5 volt (not 3.3 volt) EDO (extended data out) memory for this machine.  The C600X/280 will take full advantage of EDO DIMMs.

Memory system is non-interleaved.

Manufactured by UMAX Computer Corporation
Toll-free tech support at 1-888-600-4400
Online system support at www.supermac.com