The Money Magazine Edition

One SIMM socket.

Comes with 1024K ROMs and an Apple 1.44MB SuperDrive.

Serial Port with the phone icon supports synchronous modems, with handshaking on both output and input supported.

Sound output is 16-bit stereo for CD playthrough.  Sound output is 8-bit for Macintosh generated sounds.  Front headphone jack is 16-bit stereo.

Has an internal IDE drive with external SCSI support.

Has an international power supply.

Has a Communication Slot for network cards and modems.

Has a Video System Slot for a video capture card.

Has a Video/TV System Slot for a cable-ready television tuner.

Has a 32-bit 030 LC Processor Direct Slot (PDS).