Random Echo Data

MacPing will construct echo packets whose data consist of random values. Each echo packet MacPing sends will contain different data. Select Random Echo or Random ICMP Echo from the Probe Type pop-up menu. Enter the length of the data to be sent in each packet.