BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Calcomp 960, 1043, 1044 series         --
--                          plotters                                   --
-------------------------------------------------------------------------
-- 07-25-91  ALA - Change default port to COM2 
-- 05-23-88  ALA - Change the limits to actual plotter units.
-- 05-05-88  SJO - Removed double space in paper size word string
-- 07-21-87  KMM - Updated paper sizes
-- 07-17-87  TT  - Set COM1 as release port
-- 07-15-87  TT  - Changed largest number of pens from 4 to 8 as per Khaled
-- 07-06-87  TT  - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 2  -- communications port number

1  'A B C D E A4 A3 A2 A1 A0  ' --PAPER SIZE WORDS (must have space at end)

--Rotation flag [0=no rotation , 1=90 degrees rotation].
105 0 0 0 0 0  0  0  0  0  0

--PAPER SIZES
--201          0       0   4572    3000   --A
--202          0       0   7620    4572   --B
--203          0       0  10160    7620   --C
--204          0       0  16510   10414   --D
--205          0       0  21463   16200   --E 
--206          0       0   2794    4826   --A4
--207          0       0   6350    4826   --A3
--208          0       0   6858   10871   --A2
--209          0       0   15113  10871   --A1
--210          0       0   22225  15748   --A0
201          0       0   18288   13208  --A
202          0       0   30480   18288  --B
203          0       0   40640   30480  --C
204          0       0   65024   40640  --D
205          0       0   85852   65024  --E 
206          0       0   11176   19304  --A4
207          0       0   25400   19304  --A3
208          0       0   27432   43484  --A2
209          0       0   60452   43484  --A1
210          0       0   88900   62992  --A0

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  8  1  1

--    +-----+--X,Y PLOTTER UNITS PER INCH
--    |     |
--    V     V
103 2032  2032

--MAX PEN SPEED
104  30

END DDIF
END
