BEGIN DDIF

------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for IBM Color Graphics Adaptor display    --
--                          controller board                          --
--                                                                    --
------------------------------------------------------------------------

--      + --- XHair flag
--      |  
--      V  
101     1  

--	Color pallete

102   8 12 10  9 14 11 13  7  0  4  2  1  6  3  5  15
-- 102   8 4  2  1  6  3  5  7 0 12 10  9 14 11 13 15
-- 102 0 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15

--    +-----+-- X,Y Screen pixels per inch
--    V     V
301 67.37 27.87

--   GRAPHICS DRIVER CONFIG FLAGS.
--  *** DO NOT CHANGE THIS LINE ***
--  0 in a line number field means not used.
--    +-------------------------------- 0 = low res   ,  1 = high res.
--    |    +--------------------------- Color lookup table line number
--    |    |    +---------------------- Start shade color table line number
--    |    |    |    +----------------- Dark shade color table line number
--    |    |    |    |    +------------ Light shade color table line number
--    |    |    |    |    |    +------- Number of dsplist 16k's line number
--    |    |    |    |    |    |    +-- Dsplist o/f file name line number
--    |    |    |    |    |    |    |
120   0  102    0    0    0    0    0

END DDIF
END
