BEGIN DDIF

-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Kurta Series Three 24 inch x 24 inch   --
--                          or 18 inch x 24 inch digitizing tablet     --
--                                                                     --
-------------------------------------------------------------------------
--05-13-91 JCM Added choice of 18x24 or 24x24 inch tablet (many requests.)
--03/20/89 SJO Changed to 6 byte format
--05/04/88 PLC Add the parity flag.
--07-17-87 SJO Changed Input Loop Counter from 400 to 800 for 80386 machines
--07-02-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

--- Input Device Driver ---

--    +-- Digitizer input wait loop counter
--    |  +-- Number of digitizer units to consider as a cursor change
--    |  |     (Increase this number if the cursor 'jiggles' on the screen)
--    |  | +-- Digitizer number of push buttons to validate PB
--    |  | | +-- Digitizer number of buttons on stylus
--    |  | | |   +-- Digitizer units per inch (resolution)
--    |  | | |   |    (Normally 200 = 5 byte format, 1000 = 6 byte format)
--    |  | | |   |    +-----+-- Digitizer X,Y active area in digitizer units
--    |  | | |   |    |     |     (Active area for tablet menu)
--    |  | | |   |    |     |    +-- Digitizer RTS flag
--    |  | | |   |    |     |    |  +-- Digitizer 5/6 byte format
--    |  | | |   |    |     |    |  |     (6 byte format returns 4 byte coords)
--    |  | | |   |    |     |    |  |     (5 byte format returns 2 byte coords)
--    |  | | |   |    |     |    |  |  +-- COM port to use (1 or 2)
--    |  | | |   |    |     |    |  |  |  + PARITY (0=disable,1=odd)
--    V  V V V   V    V     V    V  V  V  V
101 800  1 2 1 1000 24000 24000  1  6  1  0  -- 24 x 24 inch tablet
--101 800  1 2 1 1000 24000 18000  1  6  1  0  -- 18 x 24 inch tablet

END DDIF
END

