--                      DLISTOFF.DEF

-- The information provided to the Vermont Microsystems Driver by this file
-- is as follows:
--      1. Entry 101: The cursor character value, 95.
--      2. Entry 103: Display List saving is NOT implemented, 0.

-- The complete list of data that could be provided to the Device Driver is
-- shown with the entry written as a comment and example if it is not 
-- implemented. 
-- The reason data is not provided for the Device Driver is because the 
-- Driver already contains default values. 
-- If the CV user wants to change the default values, then the
-- corresponding data may be initialized accordingly.


BEGIN DDIF

-- RGB color table values. Read by cv_sload.
   2 "100 600 060 006 660 067 606 667 333 900 090 009 880 09A A0A 999"

-- Starting RGB values for the shading color table. Read by cv_sload.
   3 "000 800 080 008 880 088 808 000"

-- RGB increments for the dark shades of each color. Read by cv_sload.
   4 "111 100 010 001 110 011 101 111"

-- RGB increments for the light shades of each color. Read by cv_sload.
   5 "111 011 101 110 001 100 010 111"

-- Cursor Char number. Read by cv_iload.
   101 95

-- Up to 8 text font patterns. Read by cv_iload.
   102  6168  4080  8184  32742  32663  15420  15  26214

-- 103 
-- Dlist NOT implemented. Read by cv_iload.
   104 0

-- X and Y pixels per inch. Read by cv_rload.
   301 99.0 98.0

END DDIF

END

--.DIF version = 100 
--
-- DLISTON.DIF defines Display List saving to be ON by setting entry 
-- 103 to 1. 
-- All other entries are the same as DLISTOFF.DIF.

BEGIN DDIF

-- 1. Not implemented. Command echo file name.
    2 "100 600 060 006 660 067 606 667 333 900 090 009 880 09A A0A 999"
    3 "000 800 080 008 880 088 808 000"
    4 "111 100 010 001 110 011 101 111"
    5 "111 011 101 110 001 100 010 111"
  101 95
  102 0
  103 1

--   GRAPHICS DRIVER CONFIG FLAGS.
--  *** DO NOT CHANGE THIS LINE ***
--  0 in a line number field means not used.
--    +-------------------------------- 0 = low res   ,  1 = high res.
--    |    +--------------------------- Color lookup table line number
--    |    |    +---------------------- Start shade color table line number
--    |    |    |    +----------------- Dark shade color table line number
--    |    |    |    |    +------------ Light shade color table line number
--    |    |    |    |    |    +------- Number of dsplist 16k's line number
--    |    |    |    |    |    |    +-- Dsplist o/f file name line number
--    |    |    |    |    |    |    |
120   1    2    3    4    5    0    0

END DDIF
END
